Notes Res-SIM – 10/29/2012

Best way to represent irrigation at north santiam diversion information? The dataset consistently adds 73 cfs to the minimum outflow from Apr to Oct, except during deficit years, when nothing is added.

**Should I make something conditional on type of water year especially for this rule?**

Placeholder for now adds 73cfs from Apr to Oct.

Op temp control-spillway – depends on both date and current outflow. Applies only to spillway.

Op temp control-upperRO– depends on both date and current outflow. Applies only to upperRO.

Conditional block in flood control. Columns in rule priority file below.

Column 1 – Fall or Winter normal flood ops

Column 4 – Spring or Summer flood ops

Column 5 – Flood ops if special curves have been initiated.

**May need to ignore gate-specific rules during iteration 1.**