Notes on Hills Creek – 10/26/2012

There is no documentation or information about the rule labeled Tandem – HCR and LOP. Will need to revisit this during calibration.

The following rules pertain to one particular outlet only:

Max\_HCR\_power\_release – power plant

Min\_HCR\_power – power plant

Min\_Low\_Turbine\_Flows\_at\_Low\_Reservoir\_Elevations – power plant

Min\_RO\_Flow – Regulating outlet

May need to revisit these rules if issue arise before outflow is split between the gates.