Notes – 10/26/2012

May need to temporarily disable these rules:

Max\_LOP\_max\_power\_release only concerns flow through the power house;

Max\_No\_RO\_use\_above\_900ft only concerns flow through the regulating outlet.

Until the outflow is split between available gates (spillway, powerhouse, RO), these rules will produce poor results.