Notes Foster rules – 10/26/2012

The following rules apply to a specific outlet:

Max\_FOS\_power\_release – power plant

Fish Weir Spill – spillway

Conditional block in the flood control rules at Foster. Column 1 will contain the rules for “Normal conditions downstream).

Column 4 will contain the rules for “exceeding BF downstream”. (SS at Waterloo >=18000cfs, SS at Jefferson >= 35000cfs).

Conditional block for conservation rules at Foster:

Column 2 wil contain the rules for “Green Peter above buffer zone”.

At this time, I will not include rule (only one) for cases when Green Peter is below the buffer zone. Will revisit when buffer zones are outlined for all the reservoirs.